From fc141319027485a7cfcbae2451b048ddc6c33b48 Mon Sep 17 00:00:00 2001
From: "H.J. Lu" <hjl.tools@gmail.com>
Date: Wed, 28 Jul 2021 10:42:47 -0700
Subject: [PATCH] x86: Simplify check for distinct TMM register operands

If any pair of operands in AMX instructions with 3 TMM register operands
are the same, the instruction will UD.  Don't call register_number to
check for distinct TMM register operands since all TMM register operands
have the same size.

	* config/tc-i386.c (check_VecOperands): Remove register_number
	call when checking for distinct TMM register operands.

diff --git a/gas/config/tc-i386.c b/gas/config/tc-i386.c
index d98c6c4e949..1235c3e7733 100644
--- a/gas/config/tc-i386.c
+++ b/gas/config/tc-i386.c
@@ -6076,21 +6076,16 @@ check_VecOperands (const insn_template *t)
 	}
     }
 
-  /* For AMX instructions with three tmmword operands, all tmmword operand must be
-     distinct */
-  if (t->operand_types[0].bitfield.tmmword
-      && i.reg_operands == 3)
-    {
-      if (register_number (i.op[0].regs)
-          == register_number (i.op[1].regs)
-          || register_number (i.op[0].regs)
-             == register_number (i.op[2].regs)
-          || register_number (i.op[1].regs)
-             == register_number (i.op[2].regs))
-	{
-	  i.error = invalid_tmm_register_set;
-	  return 1;
-	}
+  /* For AMX instructions with 3 TMM register operands, all operands
+      must be distinct.  */
+  if (i.reg_operands == 3
+      && t->operand_types[0].bitfield.tmmword
+      && (i.op[0].regs == i.op[1].regs
+          || i.op[0].regs == i.op[2].regs
+          || i.op[1].regs == i.op[2].regs))
+    {
+      i.error = invalid_tmm_register_set;
+      return 1;
     }
 
   /* Check if broadcast is supported by the instruction and is applied
-- 
2.33.0

