From 744fd4126937b7f195fac38ae24cab52d0922b04 Mon Sep 17 00:00:00 2001
From: David Marchand <david.marchand@redhat.com>
Date: Thu, 17 Feb 2022 14:06:14 +0100
Subject: [PATCH] net/af_xdp: add missing trailing newline in logs

[ upstream commit 744fd4126937b7f195fac38ae24cab52d0922b04 ]

Caught while trying --in-memory mode, some log messages in this driver
are not terminated with a newline:
rte_pmd_af_xdp_probe(): net_af_xdp: Failed to register multi-process IPC
callback: Operation not supportedvdev_probe(): failed to initialize
net_af_xdp device

Other locations in this driver had the same issue, fix all at once.

Fixes: f1debd77efaf ("net/af_xdp: introduce AF_XDP PMD")
Fixes: d8a210774e1d ("net/af_xdp: support unaligned umem chunks")
Fixes: 9876cf8316b3 ("net/af_xdp: re-enable secondary process support")
Cc: stable@dpdk.org

Signed-off-by: David Marchand <david.marchand@redhat.com>
Acked-by: Ciara Loftus <ciara.loftus@intel.com>
---
 drivers/net/af_xdp/rte_eth_af_xdp.c | 12 ++++++------
 1 file changed, 6 insertions(+), 6 deletions(-)

diff --git a/drivers/net/af_xdp/rte_eth_af_xdp.c b/drivers/net/af_xdp/rte_eth_af_xdp.c
index 2163df7c5c..69dfa1b898 100644
--- a/drivers/net/af_xdp/rte_eth_af_xdp.c
+++ b/drivers/net/af_xdp/rte_eth_af_xdp.c
@@ -1071,7 +1071,7 @@ xsk_umem_info *xdp_umem_configure(struct pmd_internals *internals,
 		umem = rte_zmalloc_socket("umem", sizeof(*umem), 0,
 					  rte_socket_id());
 		if (umem == NULL) {
-			AF_XDP_LOG(ERR, "Failed to allocate umem info");
+			AF_XDP_LOG(ERR, "Failed to allocate umem info\n");
 			return NULL;
 		}
 
@@ -1084,7 +1084,7 @@ xsk_umem_info *xdp_umem_configure(struct pmd_internals *internals,
 		ret = xsk_umem__create(&umem->umem, base_addr, umem_size,
 				&rxq->fq, &rxq->cq, &usr_config);
 		if (ret) {
-			AF_XDP_LOG(ERR, "Failed to create umem");
+			AF_XDP_LOG(ERR, "Failed to create umem\n");
 			goto err;
 		}
 		umem->buffer = base_addr;
@@ -1124,7 +1124,7 @@ xsk_umem_info *xdp_umem_configure(struct pmd_internals *internals,
 
 	umem = rte_zmalloc_socket("umem", sizeof(*umem), 0, rte_socket_id());
 	if (umem == NULL) {
-		AF_XDP_LOG(ERR, "Failed to allocate umem info");
+		AF_XDP_LOG(ERR, "Failed to allocate umem info\n");
 		return NULL;
 	}
 
@@ -1160,7 +1160,7 @@ xsk_umem_info *xdp_umem_configure(struct pmd_internals *internals,
 			       &usr_config);
 
 	if (ret) {
-		AF_XDP_LOG(ERR, "Failed to create umem");
+		AF_XDP_LOG(ERR, "Failed to create umem\n");
 		goto err;
 	}
 	umem->mz = mz;
@@ -1847,7 +1847,7 @@ afxdp_mp_request_fds(const char *name, struct rte_eth_dev *dev)
 	AF_XDP_LOG(DEBUG, "Sending multi-process IPC request for %s\n", name);
 	ret = rte_mp_request_sync(&request, &replies, &timeout);
 	if (ret < 0 || replies.nb_received != 1) {
-		AF_XDP_LOG(ERR, "Failed to request fds from primary: %d",
+		AF_XDP_LOG(ERR, "Failed to request fds from primary: %d\n",
 			   rte_errno);
 		return -1;
 	}
@@ -1996,7 +1996,7 @@ rte_pmd_af_xdp_probe(struct rte_vdev_device *dev)
 	if (!afxdp_dev_count) {
 		ret = rte_mp_action_register(ETH_AF_XDP_MP_KEY, afxdp_mp_send_fds);
 		if (ret < 0 && rte_errno != ENOTSUP) {
-			AF_XDP_LOG(ERR, "%s: Failed to register multi-process IPC callback: %s",
+			AF_XDP_LOG(ERR, "%s: Failed to register multi-process IPC callback: %s\n",
 				   name, strerror(rte_errno));
 			return -1;
 		}
-- 
2.33.0

