From 283338986c32000d7e145e2fa6e4d9fb2b973cfd Mon Sep 17 00:00:00 2001
From: Chengwen Feng <fengchengwen@huawei.com>
Date: Thu, 21 Dec 2023 09:12:26 +0800
Subject: [PATCH] net/hns3: don't support QinQ insert for VF

In the HIP08 platform, the PF driver will notify VF driver to update
the PVID state [1], and VF will declare support QinQ insert when PVID
is disabled.

In the later platform (e.g. HIP09), the hardware has been improved,
so the PF driver will NOT notify VF driver to update the PVID state.

However, the later platform still have constraint: PVID and QinQ insert
cannot be enabled at the same time, otherwise, the hardware discards
packets and reports an error interrupt.

Plus, as far as we known, VF driver's users don't use the QinQ insert.

Therefore, we declare that the VF driver don't support QinQ insert.

[1] commit b4e4d7ac9f09 ("net/hns3: support setting VF PVID by PF driver")

Cc: stable@dpdk.org

Signed-off-by: Chengwen Feng <fengchengwen@huawei.com>
---
 drivers/net/hns3/hns3_common.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/drivers/net/hns3/hns3_common.c b/drivers/net/hns3/hns3_common.c
index 0d6b2c65af..717649f259 100644
--- a/drivers/net/hns3/hns3_common.c
+++ b/drivers/net/hns3/hns3_common.c
@@ -85,7 +85,7 @@ hns3_dev_infos_get(struct rte_eth_dev *eth_dev, struct rte_eth_dev_info *info)
 				 RTE_ETH_TX_OFFLOAD_MBUF_FAST_FREE |
 				 RTE_ETH_TX_OFFLOAD_VLAN_INSERT);
 
-	if (!hw->port_base_vlan_cfg.state)
+	if (!hns->is_vf && !hw->port_base_vlan_cfg.state)
 		info->tx_offload_capa |= RTE_ETH_TX_OFFLOAD_QINQ_INSERT;
 
 	if (hns3_dev_get_support(hw, OUTER_UDP_CKSUM))
-- 
2.41.0.windows.2

