From 7fc6ae50369d75b9aa550072182fa92f8c4e13a4 Mon Sep 17 00:00:00 2001
From: Shibin Koikkara Reeny <shibin.koikkara.reeny@intel.com>
Date: Wed, 15 Feb 2023 16:30:14 +0000
Subject: [PATCH] net/af_xdp: support CNI Integration

[ upstream commit 7fc6ae50369d75b9aa550072182fa92f8c4e13a4 ]

Integrate support for the AF_XDP CNI and device plugin [1] so that the
DPDK AF_XDP PMD can work in an unprivileged container environment.

Part of the AF_XDP PMD initialization process involves loading an eBPF
program onto the given netdev. This operation requires privileges, which
prevents the PMD from being able to work in an unprivileged container
(without root access). The plugin CNI handles the program loading. CNI
open Unix Domain Socket (UDS) and waits listening for a client to make
requests over that UDS. The client(DPDK) connects and a "handshake"
occurs, then the File Descriptor which points to the XSKMAP associated
with the loaded eBPF program is handed over to the client. The client
can then proceed with creating an AF_XDP socket and inserting the socket
into the XSKMAP pointed to by the FD received on the UDS.

A new vdev arg "use_cni" is created to indicate user wishes to run
the PMD in unprivileged mode and to receive the XSKMAP FD from the CNI.

When this flag is set, the XSK_LIBBPF_FLAGS__INHIBIT_PROG_LOAD libbpf
flag should be used when creating the socket, which tells libbpf not to
load the default libbpf program on the netdev. We tell libbpf not to do
this because the loading is handled by the CNI in this scenario.

Patch include howto doc explain how to configure AF_XDP CNI to working
with DPDK.

[1]: https://github.com/intel/afxdp-plugins-for-kubernetes

Signed-off-by: Shibin Koikkara Reeny <shibin.koikkara.reeny@intel.com>
Tested-by: Anatoly Burakov <anatoly.burakov@intel.com>
Reviewed-by: Qi Zhang <qi.z.zhang@intel.com>
Acked-by: John McNamara <john.mcnamara@intel.com>
Acked-by: Ferruh Yigit <ferruh.yigit@amd.com>
---
 doc/guides/howto/af_xdp_cni.rst     | 255 ++++++++++++++++++++
 doc/guides/howto/index.rst          |   1 +
 drivers/net/af_xdp/rte_eth_af_xdp.c | 349 +++++++++++++++++++++++++++-
 3 files changed, 613 insertions(+), 11 deletions(-)
 create mode 100644 doc/guides/howto/af_xdp_cni.rst

diff --git a/doc/guides/howto/af_xdp_cni.rst b/doc/guides/howto/af_xdp_cni.rst
new file mode 100644
index 0000000000..a38f02450e
--- /dev/null
+++ b/doc/guides/howto/af_xdp_cni.rst
@@ -0,0 +1,255 @@
+.. SPDX-License-Identifier: BSD-3-Clause
+   Copyright(c) 2023 Intel Corporation.
+
+Using a CNI with the AF_XDP driver
+==================================
+
+Introduction
+------------
+
+CNI, the Container Network Interface, is a technology for configuring
+container network interfaces
+and which can be used to setup Kubernetes networking.
+AF_XDP is a Linux socket Address Family that enables an XDP program
+to redirect packets to a memory buffer in userspace.
+
+This document explains how to enable the `AF_XDP Plugin for Kubernetes`_ within
+a DPDK application using the `AF_XDP PMD`_ to connect and use these technologies.
+
+.. _AF_XDP Plugin for Kubernetes: https://github.com/intel/afxdp-plugins-for-kubernetes
+
+
+Background
+----------
+
+The standard `AF_XDP PMD`_ initialization process involves loading an eBPF program
+onto the kernel netdev to be used by the PMD.
+This operation requires root or escalated Linux privileges
+and thus prevents the PMD from working in an unprivileged container.
+The AF_XDP CNI plugin handles this situation
+by providing a device plugin that performs the program loading.
+
+At a technical level the CNI opens a Unix Domain Socket and listens for a client
+to make requests over that socket.
+A DPDK application acting as a client connects and initiates a configuration "handshake".
+The client then receives a file descriptor which points to the XSKMAP
+associated with the loaded eBPF program.
+The XSKMAP is a BPF map of AF_XDP sockets (XSK).
+The client can then proceed with creating an AF_XDP socket
+and inserting that socket into the XSKMAP pointed to by the descriptor.
+
+The EAL vdev argument ``use_cni`` is used to indicate that the user wishes
+to run the PMD in unprivileged mode and to receive the XSKMAP file descriptor
+from the CNI.
+When this flag is set,
+the ``XSK_LIBBPF_FLAGS__INHIBIT_PROG_LOAD`` libbpf flag
+should be used when creating the socket
+to instruct libbpf not to load the default libbpf program on the netdev.
+Instead the loading is handled by the CNI.
+
+.. _AF_XDP PMD: https://doc.dpdk.org/guides/nics/af_xdp.html
+
+.. note::
+
+   The Unix Domain Socket file path appear in the end user is "/tmp/afxdp.sock".
+
+
+Prerequisites
+-------------
+
+Docker and container prerequisites:
+
+* Set up the device plugin
+  as described in the instructions for `AF_XDP Plugin for Kubernetes`_.
+
+* The Docker image should contain the libbpf and libxdp libraries,
+  which are dependencies for AF_XDP,
+  and should include support for the ``ethtool`` command.
+
+* The Pod should have enabled the capabilities ``CAP_NET_RAW`` and ``CAP_BPF``
+  for AF_XDP along with support for hugepages.
+
+* Increase locked memory limit so containers have enough memory for packet buffers.
+  For example:
+
+  .. code-block:: console
+
+     cat << EOF | sudo tee /etc/systemd/system/containerd.service.d/limits.conf
+     [Service]
+     LimitMEMLOCK=infinity
+     EOF
+
+* dpdk-testpmd application should have AF_XDP feature enabled.
+
+  For further information see the docs for the: :doc:`../../nics/af_xdp`.
+
+
+Example
+-------
+
+Howto run dpdk-testpmd with CNI plugin:
+
+* Clone the CNI plugin
+
+  .. code-block:: console
+
+     # git clone https://github.com/intel/afxdp-plugins-for-kubernetes.git
+
+* Build the CNI plugin
+
+  .. code-block:: console
+
+     # cd afxdp-plugins-for-kubernetes/
+     # make build
+
+  .. note::
+
+     CNI plugin has a dependence on the config.json.
+
+  Sample Config.json
+
+  .. code-block:: json
+
+     {
+        "logLevel":"debug",
+        "logFile":"afxdp-dp-e2e.log",
+        "pools":[
+           {
+              "name":"e2e",
+              "mode":"primary",
+              "timeout":30,
+              "ethtoolCmds" : ["-L -device- combined 1"],
+              "devices":[
+                 {
+                    "name":"ens785f0"
+                 }
+              ]
+           }
+        ]
+     }
+
+  For further reference please use the `config.json`_
+
+  .. _config.json: https://github.com/intel/afxdp-plugins-for-kubernetes/blob/v0.0.2/test/e2e/config.json
+
+* Create the Network Attachment definition
+
+  .. code-block:: console
+
+     # kubectl create -f nad.yaml
+
+  Sample nad.yml
+
+  .. code-block:: yaml
+
+      apiVersion: "k8s.cni.cncf.io/v1"
+      kind: NetworkAttachmentDefinition
+      metadata:
+        name: afxdp-e2e-test
+        annotations:
+          k8s.v1.cni.cncf.io/resourceName: afxdp/e2e
+      spec:
+        config: '{
+            "cniVersion": "0.3.0",
+            "type": "afxdp",
+            "mode": "cdq",
+            "logFile": "afxdp-cni-e2e.log",
+            "logLevel": "debug",
+            "ipam": {
+              "type": "host-local",
+              "subnet": "192.168.1.0/24",
+              "rangeStart": "192.168.1.200",
+              "rangeEnd": "192.168.1.216",
+              "routes": [
+                { "dst": "0.0.0.0/0" }
+              ],
+              "gateway": "192.168.1.1"
+            }
+          }'
+
+  For further reference please use the `nad.yaml`_
+
+  .. _nad.yaml: https://github.com/intel/afxdp-plugins-for-kubernetes/blob/v0.0.2/test/e2e/nad.yaml
+
+* Build the Docker image
+
+  .. code-block:: console
+
+     # docker build -t afxdp-e2e-test -f Dockerfile .
+
+  Sample Dockerfile:
+
+  .. code-block:: console
+
+     FROM ubuntu:20.04
+     RUN apt-get update -y
+     RUN apt install build-essential libelf-dev -y
+     RUN apt-get install iproute2  acl -y
+     RUN apt install python3-pyelftools ethtool -y
+     RUN apt install libnuma-dev libjansson-dev libpcap-dev net-tools -y
+     RUN apt-get install clang llvm -y
+     COPY ./libbpf<version>.tar.gz /tmp
+     RUN cd /tmp && tar -xvmf libbpf<version>.tar.gz && cd libbpf/src && make install
+     COPY ./libxdp<version>.tar.gz /tmp
+     RUN cd /tmp && tar -xvmf libxdp<version>.tar.gz && cd libxdp && make install
+
+  .. note::
+
+     All the files that need to COPY-ed should be in the same directory as the Dockerfile
+
+* Run the Pod
+
+  .. code-block:: console
+
+     # kubectl create -f pod.yaml
+
+  Sample pod.yaml:
+
+  .. code-block:: yaml
+
+     apiVersion: v1
+     kind: Pod
+     metadata:
+       name: afxdp-e2e-test
+       annotations:
+         k8s.v1.cni.cncf.io/networks: afxdp-e2e-test
+     spec:
+       containers:
+       - name: afxdp
+         image: afxdp-e2e-test:latest
+         imagePullPolicy: Never
+         env:
+         - name: LD_LIBRARY_PATH
+           value: /usr/lib64/:/usr/local/lib/
+         command: ["tail", "-f", "/dev/null"]
+         securityContext:
+          capabilities:
+             add:
+               - CAP_NET_RAW
+               - CAP_BPF
+         resources:
+           requests:
+             hugepages-2Mi: 2Gi
+             memory: 2Gi
+             afxdp/e2e: '1'
+           limits:
+             hugepages-2Mi: 2Gi
+             memory: 2Gi
+             afxdp/e2e: '1'
+
+  For further reference please use the `pod.yaml`_
+
+  .. _pod.yaml: https://github.com/intel/afxdp-plugins-for-kubernetes/blob/v0.0.2/test/e2e/pod-1c1d.yaml
+
+* Run DPDK with a command like the following:
+
+  .. code-block:: console
+
+     kubectl exec -i <Pod name> --container <containers name> -- \
+           /<Path>/dpdk-testpmd -l 0,1 --no-pci \
+           --vdev=net_af_xdp0,use_cni=1,iface=<interface name> \
+           -- --no-mlockall --in-memory
+
+For further reference please use the `e2e`_ test case in `AF_XDP Plugin for Kubernetes`_
+
+  .. _e2e: https://github.com/intel/afxdp-plugins-for-kubernetes/tree/v0.0.2/test/e2e
diff --git a/doc/guides/howto/index.rst b/doc/guides/howto/index.rst
index bf6337d021..71a3381c36 100644
--- a/doc/guides/howto/index.rst
+++ b/doc/guides/howto/index.rst
@@ -8,6 +8,7 @@ HowTo Guides
     :maxdepth: 2
     :numbered:
 
+    af_xdp_cni
     lm_bond_virtio_sriov
     lm_virtio_vhost_user
     flow_bifurcation
diff --git a/drivers/net/af_xdp/rte_eth_af_xdp.c b/drivers/net/af_xdp/rte_eth_af_xdp.c
index 38b9d36ab5..02c874d51e 100644
--- a/drivers/net/af_xdp/rte_eth_af_xdp.c
+++ b/drivers/net/af_xdp/rte_eth_af_xdp.c
@@ -7,6 +7,7 @@
 #include <string.h>
 #include <netinet/in.h>
 #include <net/if.h>
+#include <sys/un.h>
 #include <sys/socket.h>
 #include <sys/ioctl.h>
 #include <linux/if_ether.h>
@@ -82,6 +83,23 @@ RTE_LOG_REGISTER_DEFAULT(af_xdp_logtype, NOTICE);
 
 #define ETH_AF_XDP_MP_KEY "afxdp_mp_send_fds"
 
+#define MAX_LONG_OPT_SZ			64
+#define UDS_MAX_FD_NUM			2
+#define UDS_MAX_CMD_LEN			64
+#define UDS_MAX_CMD_RESP		128
+#define UDS_XSK_MAP_FD_MSG		"/xsk_map_fd"
+#define UDS_SOCK			"/tmp/afxdp.sock"
+#define UDS_CONNECT_MSG			"/connect"
+#define UDS_HOST_OK_MSG			"/host_ok"
+#define UDS_HOST_NAK_MSG		"/host_nak"
+#define UDS_VERSION_MSG			"/version"
+#define UDS_XSK_MAP_FD_MSG		"/xsk_map_fd"
+#define UDS_XSK_SOCKET_MSG		"/xsk_socket"
+#define UDS_FD_ACK_MSG			"/fd_ack"
+#define UDS_FD_NAK_MSG			"/fd_nak"
+#define UDS_FIN_MSG			"/fin"
+#define UDS_FIN_ACK_MSG			"/fin_ack"
+
 static int afxdp_dev_count;
 
 /* Message header to synchronize fds via IPC */
@@ -152,6 +170,7 @@ struct pmd_internals {
 	char prog_path[PATH_MAX];
 	bool custom_prog_configured;
 	bool force_copy;
+	bool use_cni;
 	struct bpf_map *map;
 
 	struct rte_ether_addr eth_addr;
@@ -171,6 +190,7 @@ struct pmd_process_private {
 #define ETH_AF_XDP_PROG_ARG			"xdp_prog"
 #define ETH_AF_XDP_BUDGET_ARG			"busy_budget"
 #define ETH_AF_XDP_FORCE_COPY_ARG		"force_copy"
+#define ETH_AF_XDP_USE_CNI_ARG			"use_cni"
 
 static const char * const valid_arguments[] = {
 	ETH_AF_XDP_IFACE_ARG,
@@ -180,6 +200,7 @@ static const char * const valid_arguments[] = {
 	ETH_AF_XDP_PROG_ARG,
 	ETH_AF_XDP_BUDGET_ARG,
 	ETH_AF_XDP_FORCE_COPY_ARG,
+	ETH_AF_XDP_USE_CNI_ARG,
 	NULL
 };
 
@@ -1130,7 +1151,8 @@ xsk_umem_info *xdp_umem_configure(struct pmd_internals *internals,
 		ret = xsk_umem__create(&umem->umem, base_addr, umem_size,
 				&rxq->fq, &rxq->cq, &usr_config);
 		if (ret) {
-			AF_XDP_LOG(ERR, "Failed to create umem\n");
+			AF_XDP_LOG(ERR, "Failed to create umem [%d]: [%s]\n",
+				   errno, strerror(errno));
 			goto err;
 		}
 		umem->buffer = base_addr;
@@ -1315,6 +1337,245 @@ configure_preferred_busy_poll(struct pkt_rx_queue *rxq)
 	return 0;
 }
 
+static int
+init_uds_sock(struct sockaddr_un *server)
+{
+	int sock;
+
+	sock = socket(AF_UNIX, SOCK_SEQPACKET, 0);
+	if (sock < 0) {
+		AF_XDP_LOG(ERR, "Failed to opening stream socket\n");
+		return -1;
+	}
+
+	server->sun_family = AF_UNIX;
+	strlcpy(server->sun_path, UDS_SOCK, sizeof(server->sun_path));
+
+	if (connect(sock, (struct sockaddr *)server, sizeof(struct sockaddr_un)) < 0) {
+		close(sock);
+		AF_XDP_LOG(ERR, "Error connecting stream socket errno = [%d]: [%s]\n",
+			   errno, strerror(errno));
+		return -1;
+	}
+
+	return sock;
+}
+
+struct msg_internal {
+	char response[UDS_MAX_CMD_RESP];
+	int len_param;
+	int num_fds;
+	int fds[UDS_MAX_FD_NUM];
+};
+
+static int
+send_msg(int sock, char *request, int *fd)
+{
+	int snd;
+	struct iovec iov;
+	struct msghdr msgh;
+	struct cmsghdr *cmsg;
+	struct sockaddr_un dst;
+	char control[CMSG_SPACE(sizeof(*fd))];
+
+	memset(&dst, 0, sizeof(dst));
+	dst.sun_family = AF_UNIX;
+	strlcpy(dst.sun_path, UDS_SOCK, sizeof(dst.sun_path));
+
+	/* Initialize message header structure */
+	memset(&msgh, 0, sizeof(msgh));
+	memset(control, 0, sizeof(control));
+	iov.iov_base = request;
+	iov.iov_len = strlen(request);
+
+	msgh.msg_name = &dst;
+	msgh.msg_namelen = sizeof(dst);
+	msgh.msg_iov = &iov;
+	msgh.msg_iovlen = 1;
+	msgh.msg_control = control;
+	msgh.msg_controllen = sizeof(control);
+
+	/* Translate the FD. */
+	cmsg = CMSG_FIRSTHDR(&msgh);
+	cmsg->cmsg_len = CMSG_LEN(sizeof(*fd));
+	cmsg->cmsg_level = SOL_SOCKET;
+	cmsg->cmsg_type = SCM_RIGHTS;
+	memcpy(CMSG_DATA(cmsg), fd, sizeof(*fd));
+
+	/* Send the request message. */
+	do {
+		snd = sendmsg(sock, &msgh, 0);
+	} while (snd < 0 && errno == EINTR);
+
+	return snd;
+}
+
+static int
+read_msg(int sock, char *response, struct sockaddr_un *s, int *fd)
+{
+	int msglen;
+	struct msghdr msgh;
+	struct iovec iov;
+	char control[CMSG_SPACE(sizeof(*fd))];
+	struct cmsghdr *cmsg;
+
+	/* Initialize message header structure */
+	memset(&msgh, 0, sizeof(msgh));
+	iov.iov_base = response;
+	iov.iov_len = UDS_MAX_CMD_RESP;
+
+	msgh.msg_name = s;
+	msgh.msg_namelen = sizeof(*s);
+	msgh.msg_iov = &iov;
+	msgh.msg_iovlen = 1;
+	msgh.msg_control = control;
+	msgh.msg_controllen = sizeof(control);
+
+	msglen = recvmsg(sock, &msgh, 0);
+
+	/* zero length message means socket was closed */
+	if (msglen == 0)
+		return 0;
+
+	if (msglen < 0) {
+		AF_XDP_LOG(ERR, "recvmsg failed, %s\n", strerror(errno));
+		return -1;
+	}
+
+	/* read auxiliary FDs if any */
+	for (cmsg = CMSG_FIRSTHDR(&msgh); cmsg != NULL;
+			cmsg = CMSG_NXTHDR(&msgh, cmsg)) {
+		if (cmsg->cmsg_level == SOL_SOCKET &&
+				cmsg->cmsg_type == SCM_RIGHTS) {
+			memcpy(fd, CMSG_DATA(cmsg), sizeof(*fd));
+			break;
+		}
+	}
+
+	response[msglen] = '\0';
+	return msglen;
+}
+
+static int
+make_request_cni(int sock, struct sockaddr_un *server, char *request,
+		 int *req_fd, char *response, int *out_fd)
+{
+	int rval;
+
+	AF_XDP_LOG(DEBUG, "Request: [%s]\n", request);
+
+	/* if no file descriptor to send then directly write to socket.
+	 * else use sendmsg() to send the file descriptor.
+	 */
+	if (req_fd == NULL)
+		rval = write(sock, request, strlen(request));
+	else
+		rval = send_msg(sock, request, req_fd);
+
+	if (rval < 0) {
+		AF_XDP_LOG(ERR, "Write error %s\n", strerror(errno));
+		return -1;
+	}
+
+	rval = read_msg(sock, response, server, out_fd);
+	if (rval <= 0) {
+		AF_XDP_LOG(ERR, "Read error %d\n", rval);
+		return -1;
+	}
+	AF_XDP_LOG(DEBUG, "Response: [%s]\n", request);
+
+	return 0;
+}
+
+static int
+check_response(char *response, char *exp_resp, long size)
+{
+	return strncmp(response, exp_resp, size);
+}
+
+static int
+get_cni_fd(char *if_name)
+{
+	char request[UDS_MAX_CMD_LEN], response[UDS_MAX_CMD_RESP];
+	char hostname[MAX_LONG_OPT_SZ], exp_resp[UDS_MAX_CMD_RESP];
+	struct sockaddr_un server;
+	int xsk_map_fd = -1, out_fd = 0;
+	int sock, err;
+
+	err = gethostname(hostname, MAX_LONG_OPT_SZ - 1);
+	if (err)
+		return -1;
+
+	memset(&server, 0, sizeof(server));
+	sock = init_uds_sock(&server);
+
+	/* Initiates handshake to CNI send: /connect,hostname */
+	snprintf(request, sizeof(request), "%s,%s", UDS_CONNECT_MSG, hostname);
+	memset(response, 0, sizeof(response));
+	if (make_request_cni(sock, &server, request, NULL, response, &out_fd) < 0) {
+		AF_XDP_LOG(ERR, "Error in processing cmd [%s]\n", request);
+		goto err_close;
+	}
+
+	/* Expect /host_ok */
+	strlcpy(exp_resp, UDS_HOST_OK_MSG, UDS_MAX_CMD_LEN);
+	if (check_response(response, exp_resp, strlen(exp_resp)) < 0) {
+		AF_XDP_LOG(ERR, "Unexpected response [%s]\n", response);
+		goto err_close;
+	}
+	/* Request for "/version" */
+	strlcpy(request, UDS_VERSION_MSG, UDS_MAX_CMD_LEN);
+	memset(response, 0, sizeof(response));
+	if (make_request_cni(sock, &server, request, NULL, response, &out_fd) < 0) {
+		AF_XDP_LOG(ERR, "Error in processing cmd [%s]\n", request);
+		goto err_close;
+	}
+
+	/* Request for file descriptor for netdev name*/
+	snprintf(request, sizeof(request), "%s,%s", UDS_XSK_MAP_FD_MSG, if_name);
+	memset(response, 0, sizeof(response));
+	if (make_request_cni(sock, &server, request, NULL, response, &out_fd) < 0) {
+		AF_XDP_LOG(ERR, "Error in processing cmd [%s]\n", request);
+		goto err_close;
+	}
+
+	if (out_fd < 0) {
+		AF_XDP_LOG(ERR, "Error in processing cmd [%s]\n", request);
+		goto err_close;
+	}
+
+	xsk_map_fd = out_fd;
+
+	/* Expect fd_ack with file descriptor */
+	strlcpy(exp_resp, UDS_FD_ACK_MSG, UDS_MAX_CMD_LEN);
+	if (check_response(response, exp_resp, strlen(exp_resp)) < 0) {
+		AF_XDP_LOG(ERR, "Unexpected response [%s]\n", response);
+		goto err_close;
+	}
+
+	/* Initiate close connection */
+	strlcpy(request, UDS_FIN_MSG, UDS_MAX_CMD_LEN);
+	memset(response, 0, sizeof(response));
+	if (make_request_cni(sock, &server, request, NULL, response, &out_fd) < 0) {
+		AF_XDP_LOG(ERR, "Error in processing cmd [%s]\n", request);
+		goto err_close;
+	}
+
+	/* Connection close */
+	strlcpy(exp_resp, UDS_FIN_ACK_MSG, UDS_MAX_CMD_LEN);
+	if (check_response(response, exp_resp, strlen(exp_resp)) < 0) {
+		AF_XDP_LOG(ERR, "Unexpected response [%s]\n", response);
+		goto err_close;
+	}
+	close(sock);
+
+	return xsk_map_fd;
+
+err_close:
+	close(sock);
+	return -1;
+}
+
 static int
 xsk_configure(struct pmd_internals *internals, struct pkt_rx_queue *rxq,
 	      int ring_size)
@@ -1363,6 +1624,10 @@ xsk_configure(struct pmd_internals *internals, struct pkt_rx_queue *rxq,
 	cfg.bind_flags |= XDP_USE_NEED_WAKEUP;
 #endif
 
+	/* Disable libbpf from loading XDP program */
+	if (internals->use_cni)
+		cfg.libbpf_flags |= XSK_LIBBPF_FLAGS__INHIBIT_PROG_LOAD;
+
 	if (strnlen(internals->prog_path, PATH_MAX)) {
 		if (!internals->custom_prog_configured) {
 			ret = load_custom_xdp_prog(internals->prog_path,
@@ -1414,7 +1679,23 @@ xsk_configure(struct pmd_internals *internals, struct pkt_rx_queue *rxq,
 		}
 	}
 
-	if (rxq->busy_budget) {
+	if (internals->use_cni) {
+		int err, fd, map_fd;
+
+		/* get socket fd from CNI plugin */
+		map_fd = get_cni_fd(internals->if_name);
+		if (map_fd < 0) {
+			AF_XDP_LOG(ERR, "Failed to receive CNI plugin fd\n");
+			goto out_xsk;
+		}
+		/* get socket fd */
+		fd = xsk_socket__fd(rxq->xsk);
+		err = bpf_map_update_elem(map_fd, &rxq->xsk_queue_idx, &fd, 0);
+		if (err) {
+			AF_XDP_LOG(ERR, "Failed to insert unprivileged xsk in map.\n");
+			goto out_xsk;
+		}
+	} else if (rxq->busy_budget) {
 		ret = configure_preferred_busy_poll(rxq);
 		if (ret) {
 			AF_XDP_LOG(ERR, "Failed configure busy polling.\n");
@@ -1585,6 +1866,27 @@ static const struct eth_dev_ops ops = {
 	.get_monitor_addr = eth_get_monitor_addr,
 };
 
+/* CNI option works in unprivileged container environment
+ * and ethernet device functionality will be reduced. So
+ * additional customiszed eth_dev_ops struct is needed
+ * for cni. Promiscuous enable and disable functionality
+ * is removed.
+ **/
+static const struct eth_dev_ops ops_cni = {
+	.dev_start = eth_dev_start,
+	.dev_stop = eth_dev_stop,
+	.dev_close = eth_dev_close,
+	.dev_configure = eth_dev_configure,
+	.dev_infos_get = eth_dev_info,
+	.mtu_set = eth_dev_mtu_set,
+	.rx_queue_setup = eth_rx_queue_setup,
+	.tx_queue_setup = eth_tx_queue_setup,
+	.link_update = eth_link_update,
+	.stats_get = eth_stats_get,
+	.stats_reset = eth_stats_reset,
+	.get_monitor_addr = eth_get_monitor_addr,
+};
+
 /** parse busy_budget argument */
 static int
 parse_budget_arg(const char *key __rte_unused,
@@ -1705,8 +2007,8 @@ xdp_get_channels_info(const char *if_name, int *max_queues,
 
 static int
 parse_parameters(struct rte_kvargs *kvlist, char *if_name, int *start_queue,
-			int *queue_cnt, int *shared_umem, char *prog_path,
-			int *busy_budget, int *force_copy)
+		 int *queue_cnt, int *shared_umem, char *prog_path,
+		 int *busy_budget, int *force_copy, int *use_cni)
 {
 	int ret;
 
@@ -1747,6 +2049,11 @@ parse_parameters(struct rte_kvargs *kvlist, char *if_name, int *start_queue,
 	if (ret < 0)
 		goto free_kvlist;
 
+	ret = rte_kvargs_process(kvlist, ETH_AF_XDP_USE_CNI_ARG,
+				 &parse_integer_arg, use_cni);
+	if (ret < 0)
+		goto free_kvlist;
+
 free_kvlist:
 	rte_kvargs_free(kvlist);
 	return ret;
@@ -1784,8 +2091,9 @@ get_iface_info(const char *if_name,
 
 static struct rte_eth_dev *
 init_internals(struct rte_vdev_device *dev, const char *if_name,
-		int start_queue_idx, int queue_cnt, int shared_umem,
-		const char *prog_path, int busy_budget, int force_copy)
+	       int start_queue_idx, int queue_cnt, int shared_umem,
+	       const char *prog_path, int busy_budget, int force_copy,
+	       int use_cni)
 {
 	const char *name = rte_vdev_device_name(dev);
 	const unsigned int numa_node = dev->device.numa_node;
@@ -1814,6 +2122,7 @@ init_internals(struct rte_vdev_device *dev, const char *if_name,
 #endif
 	internals->shared_umem = shared_umem;
 	internals->force_copy = force_copy;
+	internals->use_cni = use_cni;
 
 	if (xdp_get_channels_info(if_name, &internals->max_queue_cnt,
 				  &internals->combined_queue_cnt)) {
@@ -1872,7 +2181,11 @@ init_internals(struct rte_vdev_device *dev, const char *if_name,
 	eth_dev->data->dev_link = pmd_link;
 	eth_dev->data->mac_addrs = &internals->eth_addr;
 	eth_dev->data->dev_flags |= RTE_ETH_DEV_AUTOFILL_QUEUE_XSTATS;
-	eth_dev->dev_ops = &ops;
+	if (!internals->use_cni)
+		eth_dev->dev_ops = &ops;
+	else
+		eth_dev->dev_ops = &ops_cni;
+
 	eth_dev->rx_pkt_burst = eth_af_xdp_rx;
 	eth_dev->tx_pkt_burst = eth_af_xdp_tx;
 	eth_dev->process_private = process_private;
@@ -1999,6 +2312,7 @@ rte_pmd_af_xdp_probe(struct rte_vdev_device *dev)
 	char prog_path[PATH_MAX] = {'\0'};
 	int busy_budget = -1, ret;
 	int force_copy = 0;
+	int use_cni = 0;
 	struct rte_eth_dev *eth_dev = NULL;
 	const char *name = rte_vdev_device_name(dev);
 
@@ -2041,11 +2355,23 @@ rte_pmd_af_xdp_probe(struct rte_vdev_device *dev)
 
 	if (parse_parameters(kvlist, if_name, &xsk_start_queue_idx,
 			     &xsk_queue_cnt, &shared_umem, prog_path,
-			     &busy_budget, &force_copy) < 0) {
+			     &busy_budget, &force_copy, &use_cni) < 0) {
 		AF_XDP_LOG(ERR, "Invalid kvargs value\n");
 		return -EINVAL;
 	}
 
+	if (use_cni && busy_budget > 0) {
+		AF_XDP_LOG(ERR, "When '%s' parameter is used, '%s' parameter is not valid\n",
+			ETH_AF_XDP_USE_CNI_ARG, ETH_AF_XDP_BUDGET_ARG);
+		return -EINVAL;
+	}
+
+	if (use_cni && strnlen(prog_path, PATH_MAX)) {
+		AF_XDP_LOG(ERR, "When '%s' parameter is used, '%s' parameter is not valid\n",
+			ETH_AF_XDP_USE_CNI_ARG, ETH_AF_XDP_PROG_ARG);
+			return -EINVAL;
+	}
+
 	if (strlen(if_name) == 0) {
 		AF_XDP_LOG(ERR, "Network interface must be specified\n");
 		return -EINVAL;
@@ -2068,8 +2394,8 @@ rte_pmd_af_xdp_probe(struct rte_vdev_device *dev)
 					busy_budget;
 
 	eth_dev = init_internals(dev, if_name, xsk_start_queue_idx,
-					xsk_queue_cnt, shared_umem, prog_path,
-					busy_budget, force_copy);
+				 xsk_queue_cnt, shared_umem, prog_path,
+				 busy_budget, force_copy, use_cni);
 	if (eth_dev == NULL) {
 		AF_XDP_LOG(ERR, "Failed to init internals\n");
 		return -1;
@@ -2129,4 +2455,5 @@ RTE_PMD_REGISTER_PARAM_STRING(net_af_xdp,
 			      "shared_umem=<int> "
 			      "xdp_prog=<string> "
 			      "busy_budget=<int> "
-			      "force_copy=<int> ");
+			      "force_copy=<int> "
+			      "use_cni=<int> ");
-- 
2.33.0

