From 785f0c94c6fa7bfbf307d2e5faa90964dca155a9 Mon Sep 17 00:00:00 2001
From: Ard Biesheuvel <ard.biesheuvel@linaro.org>
Date: Thu, 27 Feb 2020 15:12:32 +0100
Subject: [PATCH 09/13] ArmVirtPkg; avoid DxeTpmMeasurementLib in shared .DSC

DxeTpmMeasurementLib should only be used on platforms that implement
measured boot, which we will do in a future patch, but only for
ArmVirtQemu, as the remaining ones are fundamentally incompatible,
given that they do not implement a PEI phase.

So use TpmMeasurementLibNull as the default resolution for all
ArmVirtPkg platforms, regardless of how they are built.

This mirrors commit 1ec05b81e59f ("OvmfPkg: use DxeTpmMeasurementLib
if and only if TPM2_ENABLE", 2019-07-04).

Ref: https://bugzilla.tianocore.org/show_bug.cgi?id=2560
Signed-off-by: Ard Biesheuvel <ard.biesheuvel@linaro.org>
Reviewed-by: Laszlo Ersek <lersek@redhat.com>
Signed-off-by: jiangfangjie <jiangfangjie@huawei.com>
---
 ArmVirtPkg/ArmVirt.dsc.inc | 3 +--
 1 file changed, 1 insertion(+), 2 deletions(-)

diff --git a/ArmVirtPkg/ArmVirt.dsc.inc b/ArmVirtPkg/ArmVirt.dsc.inc
index 10037c9..398aa7b 100644
--- a/ArmVirtPkg/ArmVirt.dsc.inc
+++ b/ArmVirtPkg/ArmVirt.dsc.inc
@@ -165,15 +165,14 @@
   # Secure Boot dependencies
   #
 !if $(SECURE_BOOT_ENABLE) == TRUE
-  TpmMeasurementLib|SecurityPkg/Library/DxeTpmMeasurementLib/DxeTpmMeasurementLib.inf
   AuthVariableLib|SecurityPkg/Library/AuthVariableLib/AuthVariableLib.inf
 
   # re-use the UserPhysicalPresent() dummy implementation from the ovmf tree
   PlatformSecureLib|OvmfPkg/Library/PlatformSecureLib/PlatformSecureLib.inf
 !else
-  TpmMeasurementLib|MdeModulePkg/Library/TpmMeasurementLibNull/TpmMeasurementLibNull.inf
   AuthVariableLib|MdeModulePkg/Library/AuthVariableLibNull/AuthVariableLibNull.inf
 !endif
+  TpmMeasurementLib|MdeModulePkg/Library/TpmMeasurementLibNull/TpmMeasurementLibNull.inf
   VarCheckLib|MdeModulePkg/Library/VarCheckLib/VarCheckLib.inf
   UefiBootManagerLib|MdeModulePkg/Library/UefiBootManagerLib/UefiBootManagerLib.inf
 
-- 
2.18.2

