From 4af8c587a4f5b861012cb2d1ca954af8e6872162 Mon Sep 17 00:00:00 2001
From: hantwofish <hankangkang5@huawei.com>
Date: Tue, 2 Jul 2024 15:26:48 +0800
Subject: [PATCH] add flow_bifurcation switch in lstack_cfg file

---
 src/lstack/lstack.conf | 1 +
 1 file changed, 1 insertion(+)

diff --git a/src/lstack/lstack.conf b/src/lstack/lstack.conf
index c65a25d..490bdfc 100644
--- a/src/lstack/lstack.conf
+++ b/src/lstack/lstack.conf
@@ -15,6 +15,7 @@ stack_thread_mode="run-to-wakeup"
 #ltran mode need add "--map-perfect" and "--legacy-mem" in dpdk_args
 use_ltran=0
 kni_switch=0
+flow_bifurcation=0
 
 low_power_mode=0
  
-- 
2.33.0

