From 7389a936fbd5ccaae7c39d38d1440e0359f9d0e5 Mon Sep 17 00:00:00 2001
From: Peter Robinson <pbrobinson@gmail.com>
Date: Tue, 12 May 2020 08:14:26 +0100
Subject: [PATCH] rpi: Use firmware provided device tree

Signed-off-by: Peter Robinson <pbrobinson@gmail.com>
---
 configs/rpi_0_w_defconfig      | 2 +-
 configs/rpi_2_defconfig        | 2 +-
 configs/rpi_3_32b_defconfig    | 2 +-
 configs/rpi_3_b_plus_defconfig | 2 +-
 configs/rpi_3_defconfig        | 2 +-
 configs/rpi_defconfig          | 2 +-
 6 files changed, 6 insertions(+), 6 deletions(-)
 
diff --git a/configs/rpi_0_w_defconfig b/configs/rpi_0_w_defconfig
index bba5e12b12..0241f4c6d3 100644
--- a/configs/rpi_0_w_defconfig
+++ b/configs/rpi_0_w_defconfig
@@ -17,7 +17,7 @@ CONFIG_CMD_GPIO=y
 CONFIG_CMD_MMC=y
 CONFIG_CMD_USB=y
 CONFIG_CMD_FS_UUID=y
-CONFIG_OF_EMBED=y
+CONFIG_OF_BOARD=y
 CONFIG_ENV_FAT_DEVICE_AND_PART="0:1"
 CONFIG_SYS_RELOC_GD_ENV_ADDR=y
 CONFIG_ENV_VARS_UBOOT_RUNTIME_CONFIG=y
diff --git a/configs/rpi_2_defconfig b/configs/rpi_2_defconfig
index 1c2bbb29ce..9573e475f4 100644
--- a/configs/rpi_2_defconfig
+++ b/configs/rpi_2_defconfig
@@ -17,7 +17,7 @@ CONFIG_CMD_GPIO=y
 CONFIG_CMD_MMC=y
 CONFIG_CMD_USB=y
 CONFIG_CMD_FS_UUID=y
-CONFIG_OF_EMBED=y
+CONFIG_OF_BOARD=y
 CONFIG_ENV_FAT_DEVICE_AND_PART="0:1"
 CONFIG_SYS_RELOC_GD_ENV_ADDR=y
 CONFIG_ENV_VARS_UBOOT_RUNTIME_CONFIG=y
diff --git a/configs/rpi_3_32b_defconfig b/configs/rpi_3_32b_defconfig
index b8a3d17f43..252df994e6 100644
--- a/configs/rpi_3_32b_defconfig
+++ b/configs/rpi_3_32b_defconfig
@@ -18,7 +18,7 @@ CONFIG_CMD_GPIO=y
 CONFIG_CMD_MMC=y
 CONFIG_CMD_USB=y
 CONFIG_CMD_FS_UUID=y
-CONFIG_OF_EMBED=y
+CONFIG_OF_BOARD=y
 CONFIG_ENV_FAT_DEVICE_AND_PART="0:1"
 CONFIG_SYS_RELOC_GD_ENV_ADDR=y
 CONFIG_ENV_VARS_UBOOT_RUNTIME_CONFIG=y
diff --git a/configs/rpi_3_b_plus_defconfig b/configs/rpi_3_b_plus_defconfig
index 4c361438fa..3b2996a2f9 100644
--- a/configs/rpi_3_b_plus_defconfig
+++ b/configs/rpi_3_b_plus_defconfig
@@ -18,7 +18,7 @@ CONFIG_CMD_GPIO=y
 CONFIG_CMD_MMC=y
 CONFIG_CMD_USB=y
 CONFIG_CMD_FS_UUID=y
-CONFIG_OF_EMBED=y
+CONFIG_OF_BOARD=y
 CONFIG_ENV_FAT_DEVICE_AND_PART="0:1"
 CONFIG_SYS_RELOC_GD_ENV_ADDR=y
 CONFIG_ENV_VARS_UBOOT_RUNTIME_CONFIG=y
diff --git a/configs/rpi_3_defconfig b/configs/rpi_3_defconfig
index 9b281a4f15..1e9ee6122e 100644
--- a/configs/rpi_3_defconfig
+++ b/configs/rpi_3_defconfig
@@ -18,7 +18,7 @@ CONFIG_CMD_GPIO=y
 CONFIG_CMD_MMC=y
 CONFIG_CMD_USB=y
 CONFIG_CMD_FS_UUID=y
-CONFIG_OF_EMBED=y
+CONFIG_OF_BOARD=y
 CONFIG_ENV_FAT_DEVICE_AND_PART="0:1"
 CONFIG_SYS_RELOC_GD_ENV_ADDR=y
 CONFIG_ENV_VARS_UBOOT_RUNTIME_CONFIG=y
diff --git a/configs/rpi_defconfig b/configs/rpi_defconfig
index b5ad53c37b..223fc03275 100644
--- a/configs/rpi_defconfig
+++ b/configs/rpi_defconfig
@@ -17,7 +17,7 @@ CONFIG_CMD_GPIO=y
 CONFIG_CMD_MMC=y
 CONFIG_CMD_USB=y
 CONFIG_CMD_FS_UUID=y
-CONFIG_OF_EMBED=y
+CONFIG_OF_BOARD=y
 CONFIG_ENV_FAT_DEVICE_AND_PART="0:1"
 CONFIG_SYS_RELOC_GD_ENV_ADDR=y
 CONFIG_ENV_VARS_UBOOT_RUNTIME_CONFIG=y
-- 

